PWS Technical Manual – UV – Resource 1

|  |  |  |
| --- | --- | --- |
| **UV Water Disinfection Unit****Location:** |  |  |
| Month 1 Month 2 Month 3 Month 4 Month 5 Month 6 Month 7 Month 8 Month 9 Month 10 Month 11 Month 12 |
| **Date:** |  |  |  |  |  |  |  |  |  |  |  |  |

|  |
| --- |
| **Cleaning** |
| **Extent of fouling before cleaning**(Score 1- clean to 5 - filthy) |  |  |  |  |  |  |  |  |  |  |  |  |
| **Quartz sleeves cleaned (TICK)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Sensors cleaned (TICK)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Interior of chamber cleaned (TICK)** |  |  |  |  |  |  |  |  |  |  |  |  |

|  |
| --- |
| **UVT Sensor** |
| **UVT sensor reading (before cleaning)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Sensors cleaned (TICK)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **UVT sensor reading (after cleaning)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Reference sensor reading (if applic.)** |  |  |  |  |  |  |  |  |  |  |  |  |

|  |
| --- |
| **Lamps** |
| **Lamp hours run** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Lamp replaced? (TICK)**Check Mfrs recommendations |  |  |  |  |  |  |  |  |  |  |  |  |

|  |
| --- |
| **General** |
| **O-rings replaced? (TICK)** |  |  |  |  |  |  |  |  |  |  |  |  |
| **Other Maintenance / Comments** |  |  |  |  |  |  |  |  |  |  |  |  |